We first find the address of magic8ball[3][4], which is

**0x7fffffffe0e0: 0x57 0x72 0x6f 0x6e 0x67 0x00 0x00 0x00**

Since whatever in little or big endian, the method of storing characters in ASCII code is the same. Thus, it should be interpreted as “Wrong”.

The output value of magic8ball[3][4] is Wrong.